**Current List of A3Sat Commands:**

* Update callsign (replace ▯ with callsign): “avionic sett call ▯”
* Update beacon interval (replace ▯ with interval): “avionic sett beac ▯”
* Update measurement interval (replace ▯ with interval): “avionic sett meas ▯”
* Update maximum data entries (replace ▯ with max value): “avionic sett maxd ▯”
* Update maximum error entries(replace ▯ with max value): “avionic sett maxe ▯”
* Reboot the CubeSat: “avionic sett rebt”
* Reset the CubeSat configurations “avionic sett rset”
* Wipe the state, configuration, and error log: “avionic sett wipe”
* Forward message (replace ▯ with message): “avionic tran ▯”
* Sends current data: "avionic telm -c"
* Pull a specific file number (replace ▯with number): "avionic telm -s ▯"
* Ping device: "avionic ping"
* Get uptime of device (time since last reset): "avionic stat -u"
* Get monotonic time (time with continuous power): "avionic stat -m"
* Get believed UTC time: "avionic stat -t"
* Get current number of data entries: “avionic stat -d”
* Get current number of error entries: “avionic stat -e”

*We highly encourage groups to add their own commands to learn about the code and increase the functionality of the A3Sat II. If you have made a command or change that is useful, reach out to us and we could integrate it into the official version of the code.*